This is the FreeCAD simple fluid material library
data is taken from matweb
currently only water and air at the standard condition (20C and 1 atm) is prepared for testing


CSIR team is working on CfdFluidMaterial in CFD workbench to support more complex fluid material

